FRF - Setup Screen

 
Use the Up/Down arrow keys to navigate to setup settings. 

Use the RIGHT arrow key to open the selected item for editing. 
Use the FIRE key or LEFT arrow key to close the editor when the 
desired selection has been made.

Further settings are available by pressing EXPAND button.

Setup can be stored using the STORE button.

Press FIRE or START buttons to start measurement.
BACK key will return to Main Menu.
DEFAULT will return the settings to default.


Menu items:
* Response Channel(s) - Set the number of channels to collect data.
* Excitation Method - select hammer or continuous
* Hammer Units - select from N or lbf. [Hammer mode only]
* H.Sens. (mV/N) - enter hammer sensitivity
* H. ICP Power - toggle the hammer ICP power ON/OFF
* Sensor - Select from a list of pre-defined sensors or choose variable to manually set sensor.
* Sensor units - Set the measurement units used by the sensor. [Expand only]
* Sensitivity - Enter transducer sensitivity in mV per sensor unit.[Expand only]
* ICP Power - Toggle the ICP power on/off. [Expand only]
* Response Range - select the response range limit that you would expect to see
* Measurement - select Apparent Mass, Accelerance, Impedance, Mobility, Stiffness or Compliance [Hammer only] or g/g, mm/s/g or um/g [Continuous]
* Meas Units - Select the displayed units type for the measurement. 
* Y-axis - Select Y-axis scale from Linear, Log or dB. 
* Hammer Range - select the desirted range for the Hammer [Hammer mode only]
* Freq Range - select the frequency range for the measurement
* Num of Lines - Select the number of lines 
* Windowing - select Forec-Exp or Uniform for hammer mode, default is Hanning for Continuous mode
* Num. Averages - Select number of averages. [Expand only]
* Accept/Reject - select Manual or Automatic [Hammer mode only]
* Invert Phase - toggle between ON/OFF
* Good Coherance - select the % level that good coherance is set to
* Save To - select between Internal or SD card
* Posn. Autoincr - toggle between ON/OFF