Analyzer - Setup Screen

 
Use the Up/Down arrow keys to navigate to setup settings. 

Use the RIGHT arrow key to open the selected item for editing. 
Use the FIRE key or LEFT arrow key to close the editor when the 
desired selection has been made.

Further settings are available by pressing "Expand" button.

Setup can be stored using the "Save" button.

Press FIRE or "Start" buttons to start measurement.
"Back" key will return to Main Menu.
"Default" will return the settings to default.


Menu items:
* Num Channels - Set the number of channels to collect data.
* Sensor - Select from a list of pre-defined sensors or choose variable to manually set sensor.
* Sensor units - Set the measurement units used by the sensor. [Expand only]
* Sensitivity - Enter transducer sensitivity in mV per sensor unit.[Expand only]
* ICP Power - Toggle the ICP power on/off. [Expand only]
* View Signal - set the display format from Spectrum, Time, Spectrum+Time, Spectrum+Cross Phase or Orbit. [Expand only]
* Y-axis Units - Select the displayed units type for the measurement. 
* X-axis Units - select either Hz or CPM. [Expand only]
* Filter - Select High Pass filter range
* Freq Range - Select maximum frequency range
* Display Y-axis - Select Y-axis scale from Linear, Log or dB. [Expand only]
* Detection - Select from RMS, peak calculated , peak to peak calculated, True peak or True peak to peak.
* Lines - Select the number of lines 
* Avg. Type - Select averaging type from RMS, Exponential or PkHold. [Expand only]
* Num. Averages - Select number of averages. [Expand only]
* Overlap - Select % overlap. [Expand only]
* Window - select window type from Hanning, Hamming, Flat +Top or Rectangular. [Expand only]


For an Orbit, the x-axis corresponds to the Ch1 sensor position and the y-axis corresponds to the Ch2 sensor position.