Recorder - Setup Screen

 
Use the Up/Down arrow keys to navigate to setup settings. 

Use the RIGHT arrow key to open the selected item for editing. 
Use the FIRE key or LEFT arrow key to close the editor when the 
desired selection has been made.

Further settings are available by pressing EXPAND button.

Setup can be stored using the STORE button.

Press FIRE or START buttons to start measurement.
BACK key will return to Main Menu.
DEFAULT will return the settings to default.


Menu items:
* Input Channels - Set the number of channels to collect data.
* Sensor - Select from a list of pre-defined sensors or choose variable to manually set sensor.
* Sensor units - Set the measurement units used by the sensor. [Expand only]
* Sensitivity - Enter transducer sensitivity in mV per sensor unit.[Expand only]
* ICP Power - Toggle the ICP power on/off. [Expand only]
* Freq Range - Select required frequency range
* Rec. Time (s) - Sets the maximum time for recording.
* Rec. Mode - Choose whether the Recording is to be started manually, or automatically based on the Ch1 input level.
* Trig. Level - Used when 'Rec. Mode' is set to 'Ch1 Level'.