RuCd - Bode Set-up

Use the Up/Down arrow keys to navigate to setup settings. 

Use the RIGHT arrow key to open the selected item for editing. 
Use the FIRE key or LEFT arrow key to close the editor when the 
desired selection has been made.

Press FIRE or DISPLAY buttons to start measurement.
BACK key will return to Main Menu.

Menu items:
* Channel - Select the channel to be displayed
* Start Spd (RPM) - Use the alphanumeric keypad to enter the RPM start speed for the plot. By default this value is the same as the start speed set in the main setup screen. 
* Stop Spd (RPM) - Use the alphanumeric keypad to enter the RPM stop speed for the plot. By default this value is the same as the stop speed set in the main setup screen.
* Spacing - Use the drop-down menu to select the type of interval to be used for the plots. Choices available are: ΔRPM, %ΔRPM, ΔTime, ΔRPM + ΔTime or %ΔRPM + ΔTime.
Depending on which option is selected will allow you to enter values for the speed interval and time interval using the alphanumeric keypad.
* Display Units - Select the Y-axis units from the drop down menu. The available units will vary depending on the transducer used to collect the data.
* LF Cutoff - Select from the drop-down menu whether or not to apply a low frequency filter, at 0.3× the running speed. For integrated measurements it is recommended that the LF Cutoff is set to On.
* Detection - Determines signal detection and scaling from rms, pc or ppc.  
* Y-Axis - Choose whether to display the Y-axis for the magnitude trace on a linear or logarithmic scale.
* Show overall - Select from a drop-down menu whether the overall should be displayed on the plot, ON/OFF. 
* Num Traces - Select from the drop-down menu the number of traces to be displayed. If the overall is selected then a maximum of 3 traces can be displayed, otherwise the maximum is 4.
* Trace Order #1 -  Use the alphanumeric keypad to enter the order number to be displayed on this trace.
* Trace Order #2 -  Use the alphanumeric keypad to enter the order number to be displayed on this trace. This option is only available if the number of traces is 2 or more.
* Trace Order #3 -  Use the alphanumeric keypad to enter the order number to be displayed on this trace. This option is only available if the number of traces is 3 or more.
* Trace Order #4 -  Use the alphanumeric keypad to enter the order number to be displayed on this trace. This option is only available if the number of traces is 4 and the overall is switched off.
