RuCd - WAV set-up

This screen lets you set up the parameters for a WAV file which you wish to process. Only WAV files containing 2-channel data can be processed: CH1 is taken to be the vibration signal and CH2 the tacho signal.

The WAV file is automatically scanned to determine the maximum speed present: if the number of pulses-per-rev is not equal to 1.0 then enter the correct value before proceeding.

* Max M/c Speed - specifies the maximum machine speed of interest in this WAV file. Automatically preset to the highest detected m/c speed.

* Mode - Runup / Manual / Coastdown - specify the mode in which the WAV was captured. If in doubt use Manual.

* Pulses/Rev - specify the number of tacho pulses per shaft revolution. Changing this will change the Max M/c Speed setting.

* Start Spd, Stop Spd - if the mode is Runup or Coastdown, specify the approximate start and stop speeds at which the WAV file was recorded. Not applicable for Manual mode.

