Idler Monitor Admin Configuration Screen

This screen gives additional configuration options to be used if required. Normally however the defaults are satisfactory.

* Measurement Fmax: change the frequency range used for the measurements (both gSE and baseband)

* Num of Lines: change the size of the FFT used for processing.

* Min num of Orders, Max Num of Orders: change the range of multiples of idler speed which is searched for possible harmonic activity.

* Blanking: change the input level at which the "Low Signal Level" detection is enabled

* Recording: enable or disable logging of results to CSV file

* Normalisation: enable or disable normalisation functionality