Item Number: 00318ET3E182JM-W22
Manufacturer: WEG
Manufacturer Part No: 00318ET3E182JM-W22

Tech Specs		
Brand	WEG Motors	
Model Number	00318ET3E182JM-W22	
HP	3 HP	
RPM	1760	
FRAME	182JM	
VOLTAGE	460 V	
PHASE	THREE	
FREQUENCY	60 Hz	
ENCLOSURE	TEFC	
APPROXIMATE WEIGHT (lb)	90	
FEET	YES	
TERMINAL BOX	LEFT	
FLANGE	FC-149	
RATED CURRENT	3.88 A	
LOCKED ROTOR CURRENT IL IN	8.1	
LOCKED ROTOR CURRENT	31.4 A	
LOCKED ROTOR TORQUE	2.3	
BREAKDOWN TORQUE	3.4	
EFFICIENCY 50	86.5	
EFFICIENCY 75	88.5	
EFFICIENCY 100	89.5	
POWER FACTOR 50	0.61	
POWER FACTOR 75	0.73	
POWER FACTOR 100	0.79	
SERVICE FACTOR	1.25	
INERTIA KGM2	0.01433 kgm	
INERTIA SQ FT	0.34005 sq.ft.	
LOCKED ROTOR TIME	23 s	
NOISE LEVEL	56 dB(A)	
ALTITUDE	1000	
DUTY CYCLE	S1	
AMBIENT TEMPERATURE	-20C - +40C	
DEGREE OF PROTECTION	IP55	
NO-LOAD CURRENT	2.00 A	
INSULATION CLASS	F	
FULL LOAD TORQUE NM	12.0 Nm	
FULL LOAD TORQUE FT	8.83 .ft	
SLIP	0.0222	
DESIGN	B	
TEMPERATURE RISE	80 K	
BEARINGS D E	6307 ZZ	
BEARINGS N D E	6206 ZZ	
REGREASING INTERVAL D E	-	
REGREASING INTERVAL N D E	-	
GREASE AMOUNT D E	-	
GREASE AMOUNT N D E	-