Balancing - Setup Screen

 
Use the Up/Down arrow keys to navigate to setup settings. 

Use the RIGHT arrow key to open the selected item for editing. 
Use the FIRE key or LEFT arrow key to close the editor when the 
desired selection has been made.

Further settings are available by pressing EXPAND button.

Setup can be stored using the SAVE button.

Press FIRE or START buttons to start measurement.

"Back" key will return to Main Menu.
"Default" will return the settings to default.

Menu items:
* Plane Setup - Set the number of planes to collect data.
* Sensor - Select from a list of pre-defined sensors or choose variable to manually set sensor.
* Sensor units - Set the measurement units used by the sensor. [Expand only]
* Sensitivity - Enter transducer sensitivity in mV per sensor unit.[Expand only]
* ICP Power - Toggle the ICP power on/off. [Expand only]
* Display Units - Select the displayed units type for the measurement. 
* Detection - Select from RMS,peak calculated or peak to peak calculated.[Expand only]
* Weight units - Select from gr, kg, cm, mm, EU or %
* Length units - Select from mm, cm, m or EU. [Expand only]
* Trigger - Select from Automatic, Manual or Visual.
* Vib. Threshold - Use the numeric keypad to enter the vibration threshold in um. [Expand only]
* Solution - Select either Dynamic or 1-2 Plane with Prognosis (only availiable when 2 plane is selected)
* Correction Type - Select Polar, Component or Fixed Weight
